Pro Lite SXS:
The intent of the COR Pro Lite SXS class is to serve as an intermediate step between Pro AM turbo SxS competition and Pro SxS class competition. Pro Lite SXS class is a production based 1000cc forced induction class or a 2000 CC na vehicle. Vehicles must be a standard manufacturer production model that is currently available to the general public in the USA. Vehicle style must have a manufacturer production volume of at least 1000 units. All new models/brands are subject to series pre-approval process which may include (but is not limited to) inspection, track time and data collection before being deemed legal for competition. To be considered for approval for the CHAMP OFFROAD during the 2025 season, all new models must be available and on dealership floors at least 30 days before the national event it is competing in. All general rulebook rules apply to the Pro Lite SXS class unless otherwise noted below or in the class definition chart. Data logging using a GPS enabled data logger is required. Refer to class chart for legal changes/modifications. Drivers running Pro Lite SXS are not eligible for sportsman SxS class.



[bookmark: Pro_AM_Turbo_SxS_Rules:]Pro Lite SXS Rules:
· Pro Lite SXS class will use solid white numbers on a blue background with the class listed on the number plate in all 5 locations, NO LETTERS in your Bib #.
· Please refer to FIG-1 SxS cage diagram noted in general section for cage rules.
· Door areas may have the OEM plastic removed
· Weights and measures:
a. Maximum width is 82” Front and rear
b. 8” ride height
c. Maverick R minimum weight 2450lbs with driver: the weight maybe adjusted after race data is collected
d. All other cars minimum weight 1850 measured at any point pre/post-race with driver.
· Fuel System must be Completely OEM with the exception of COR approved fuel cells/OEM tanks and the change from an OEM fuel line to an aftermarket fuel line.
· Gauge cluster may be removed.
· May use aftermarket exhaust – Titanium mufflers are legal.
· Aftermarket intake may be relocated using OEM protocols the intake ports, and throttle bodies may not be modified in any way. OEM Can bus ecu boost protocols must be maintained. Intake mounting to head must maintain OEM configurations, all intakes are subject to Champ Off-Road approval and any decisions disqualifying any intakes are final and not subject to appeal.
· All wiring harnesses, ECU, Electronical controls must be OEM.
· OEM ECU only
· No OEM internal performance engine accessories are legal.
· Yamaha models may update clutch basket and springs/pressure plate/friction plates
· CVT models may update weights, springs, helix, aftermarket cvt clutches are legal.
· OEM production-based turbo cars may use any commercially available intercooler
· Carbon fiber and Titanium are prohibited from anywhere on the SxS unless specifically otherwise stated
· Aftermarket waste gate actuators are legal.
· Front and rear differentials must be from the model of vehicle used with no modification. 

Yamaha Specific Rules:
Regulated at 60psi at the rail 64psi at the pump
Data recording is mandatory measuring fuel pressure at the rail, boost at the throttle body using the unused port capped by the OEM (will have a diagram for this) failure to have an active data logger will result in a DQ
Yamaha OEM Sidewinder Injector x3 Part Number: 8KJ-13761-00-00 GYTR Cast Exhaust Manifold 2022 Spec Part number: BAS-E4602-V0 GYTR Turbo 42MM 2022 Spec Part Number: BAS-E46F2-R0
DLP Supplied Aero-motive Fuel Pump and fuel PSI regulator kit Part Number: DLPFPK 201
DLP Supplied Solenoid for Boost Control. Brand: MAC Valves. Part Number 35AA-AAA-DDBA-1BA Or
Regulated to stock base fuel pressure (3.5 bar) with boost referenced at the regulator. Boost will be logged through the datalogger via Can bus channel utilizing the factory map sensor. Failure to have an actual data logger will result in DQ
OEM Yamaha Sidewinder Piston Part Number 8KJ-11631-00-00 OEM Yamaha Sidewinder Rings Part Number 8KJ-11601-01-00 OEM Yamaha Sidewinder wrist pin Part Number 8KJ-11633-00-00
OEM Yamaha Sidewinder Connecting Rod Part Number 8KJ-11650-00-00 OEM Yamaha Sidewinder Head Gasket Part Number 8KJ-11181-00-00
DLP Supplied 580cc fuel injectors x3 - Part Number DLP-00170 DLP Supplied Exhaust Manifold with V- band mounting - Part Number DLP-00095 DLP supplied 44mm turbo and wastegate actuator - Part Number DLP-80001 DLP Supplied Aeromotive Fuel Pump and fuel PSI regulator Kit - Part Number DLP- 00143 (DLPFPK) DLP Supplied Solenoid for Boost Control, Brand: MAC Valves - Part Number DLP-80002 (35AA-AAA-DDBA-1BA)
Deviation from these parts and their respective numbers will result in a DQ
· 

